# CANBERRA COLLEGE THEATRE TECHNICAL SPECIFICATIONS

**STAGE**

**Brief Stage Description:**

Unraked stage. Soft proscenium arch with use of drapes in wings and full front stage curtains. **No Flying facilities**

White painted wall upstage can be used as rear cyclorama for projection.

Stage distributed load limit **500kg/m2**

Stage point load limit **Not Known**

Stage rake **No**

**Stage Dimensions:**

**Proscenium**

**Width 14.1m**

**Height 5.6m**

**Setting Line**

**400mm in front of house curtain**

**Distance From *(SL = Setting Line, CL = Centre Line)***

**SL to DS edge of apron 4.5m**

**SL to First wing/leg 1.8m**

**SL to Second wing/leg 3.4m**

**SL to Third wing/leg 5m**

**SL to Rear wall/cyclorama 10.9m**

**CL to OP wing/leg (or obstruction) 5.1m**

**CL to PS wing/leg (or obstruction) 5.1m**

**Total usable stage (excluding apron)**

**OP – PS = 10.2m DS – US = 6.3m**

Old dimensions can be found on (excludes the wings/legs):

<http://www.canberrac.act.edu.au/information2/performing_arts_centre>

[12-07-06\_CCPAC\_Stage\_Dims\_(2).pdf](file:///\\evsstfg.actedu.net.au\staff\stfG\CBRC\Arts\CCPAC\Documents%20for%20CCPAC%20Hirers\2013\Theatre%20Hire\12-07-06_CCPAC_Stage_Dims_(2).pdf)

**Auditorium:**

**Raked seating**

**Seating capacity with removable seating included 174**

**Seating capacity excluding removable seating 164**

**Flying facilities**

No Fly system only two FOH bridges

**Orchestra Pit**

No Orchestra Pit

Drapery: **(Fixed dead hung battens - Tormentor, house and Traveller w/ Track)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Type** | **Material** | **Colour** | **Width** | **Height** | **Quantity** | **Distance from setting line** |
| Teaser | Flat Wool | Black | 15.5m | 1.6m | 1 | 140mm |
| Tormentor | Flat Wool | Black | 2.5m | 6.8m | 1 | 240mm |
| House curtain | Velour | Royal Blue | 9m | 6.4m | 1 | 440mm |
| Borders | Flat Wool | Black | 15.4m | 1.6m | 3 | N/A |
| Legs | Flat Wool | Black | 3.8m | 6.8m | 3 | As above |
| Traveller | Flat Wool | Black | 9m | 6.8m | 1 | 6050mm |

Access Equipment:

No access equipment including ladders

Stage Covers:

N/A

Stage traps:

There are two (2) downstage traps/ dips located 4m from front edge of stage and 3.14m m from O and OP wings. Use of the floor traps must be authorised by the Technical Coordinator

Safety Curtain:

No Safety Curtain installed

Loading Dock:

**Truck access via the main school car park at the rear of CCPAC**

Loading Dock Height **Road Level**

Door Dimensions **4.4m** High

**3.5m** Wide

**Restrictions/Obstructions – A/C obstruction inside loading dock at 3.6m**