# CANBERRA COLLEGE THEATRE TECHNICAL SPECIFICATIONS

**STAGE**

 **Brief Stage Description:**

 Unraked stage. Soft proscenium arch with use of drapes in wings and full front stage curtains. **No Flying facilities**

White painted wall upstage can be used as rear cyclorama for projection.

 Stage distributed load limit **500kg/m2**

 Stage point load limit **Not Known**

 Stage rake **No**

 **Stage Dimensions:**

 **Proscenium**

 **Width 14.1m**

 **Height 5.6m**

 **Setting Line**

 **400mm in front of house curtain**

 **Distance From *(SL = Setting Line, CL = Centre Line)***

 **SL to DS edge of apron 4.5m**

 **SL to First wing/leg 1.8m**

 **SL to Second wing/leg 3.4m**

 **SL to Third wing/leg 5m**

 **SL to Rear wall/cyclorama 10.9m**

 **CL to OP wing/leg (or obstruction) 5.1m**

 **CL to PS wing/leg (or obstruction) 5.1m**

 **Total usable stage (excluding apron)**

 **OP – PS = 10.2m DS – US = 6.3m**

Old dimensions can be found on (excludes the wings/legs):

<http://www.canberrac.act.edu.au/information2/performing_arts_centre>

[12-07-06\_CCPAC\_Stage\_Dims\_(2).pdf](file:///%5C%5Cevsstfg.actedu.net.au%5Cstaff%5CstfG%5CCBRC%5CArts%5CCCPAC%5CDocuments%20for%20CCPAC%20Hirers%5C2013%5CTheatre%20Hire%5C12-07-06_CCPAC_Stage_Dims_%282%29.pdf)

 **Auditorium:**

 **Raked seating**

 **Seating capacity with removable seating included 174**

 **Seating capacity excluding removable seating 164**

 **Flying facilities**

No Fly system only two FOH bridges

 **Orchestra Pit**

No Orchestra Pit

 Drapery: **(Fixed dead hung battens - Tormentor, house and Traveller w/ Track)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Type** | **Material** | **Colour** | **Width** | **Height** | **Quantity** | **Distance from setting line** |
| Teaser | Flat Wool | Black | 15.5m | 1.6m | 1 | 140mm |
| Tormentor | Flat Wool | Black | 2.5m | 6.8m | 1 | 240mm |
| House curtain | Velour | Royal Blue | 9m | 6.4m | 1 | 440mm |
| Borders | Flat Wool  | Black | 15.4m | 1.6m | 3 | N/A |
| Legs | Flat Wool | Black | 3.8m | 6.8m | 3 | As above |
| Traveller | Flat Wool | Black | 9m | 6.8m | 1 | 6050mm |

 Access Equipment:

No access equipment including ladders

 Stage Covers:

N/A

 Stage traps:

 There are two (2) downstage traps/ dips located 4m from front edge of stage and 3.14m m from O and OP wings. Use of the floor traps must be authorised by the Technical Coordinator

 Safety Curtain:

 No Safety Curtain installed

 Loading Dock:

 **Truck access via the main school car park at the rear of CCPAC**

 Loading Dock Height **Road Level**

 Door Dimensions **4.4m** High

 **3.5m** Wide

 **Restrictions/Obstructions – A/C obstruction inside loading dock at 3.6m**